**DATCP- ATCP 50 Cost Share Program Descriptions**

**ATCP 50.62** **Manure storage systems.**

[ATCP 50.62(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.62%281%29) **(1)**  Definitions. In this section:

[ATCP 50.62(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.62%281%29%28a%29) **(a)** “Animal feeding operation" means a feedlot or facility, other than a pasture, where animals are fed, confined, maintained, or stabled for 45 days or more in any 12-month period. Two or more animal

**ATCP 50.63** **Manure storage system closure.**

[ATCP 50.63(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.63%281%29)**(1)**  Definitions. In this section:

[ATCP 50.63(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.63%281%29%28a%29) **(a)** “Manure storage system" has the meaning given in s. [ATCP 50.62 (1) (e)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.62%281%29%28e%29).

[ATCP 50.63(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.63%281%29%28b%29) **(b)** “Manure storage system closure" means permanently disabling and sealing a leaking or improperly sited manure storage system

**ATCP 50.64** **Barnyard runoff control systems.**

[ATCP 50.64(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.64%281%29)**(1)**  Definition. In this section, “barnyard runoff control system" means a system of facilities or practices used to contain, divert, retard, treat, or otherwise control the discharge of runoff from outdoor areas of concentrated livestock activity. A “barnyard runoff control system" may include any of the following components which is necessary to contain, divert, retard, treat, or control surface water runoff:

**ATCP 50.65** **Access road.**

[ATCP 50.65(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.65%281%29) **(1)**  Definition. In this section, “access road" means a road or pathway that confines or directs the movement of livestock, farm equipment, or vehicular traffic, and that is designed and installed to control surface water runoff, to protect an installed practice, or to prevent erosion.

**ATCP 50.66 Trails and walkways.**

[ATCP 50.66(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.66%281%29) **(1)**  Definition. In this section, “trail or walkway" means a travel lane to facilitate movement of livestock or people.

**ATCP 50.67** **Contour farming.**

[ATCP 50.67(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.67%281%29) **(1)**  Definition. In this section, “contour farming" means plowing, preparing, planting, and cultivating sloping land on the contour and along established grades of terraces or diversions.

**ATCP 50.68** **Cover crop.**

[ATCP 50.68(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.68%281%29) **(1)**  Definition. In this section, “cropland cover" means close-growing grasses, legumes, or small grain grown for any of the following purposes:

[ATCP 50.68(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.68%281%29%28a%29) **(a)** To control erosion during periods when major crops do not furnish adequate cover.

[ATCP 50.68(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.68%281%29%28b%29) **(b)** To add organic matter to the soil.

[ATCP 50.68(1)(c)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.68%281%29%28c%29) **(c)** To improve soil infiltration, aeration, or tilth.

**ATCP 50.69** **Critical area stabilization.**

[ATCP 50.69(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.69%281%29) **(1)**  Definition. In this section, “critical area stabilization" means planting suitable vegetation on erodible areas such as steep slopes and gullies, so as to reduce soil erosion or pollution from agricultural nonpoint sources. “Critical area stabilization" may also include treating areas that drain into bedrock crevices, openings, or sinkholes.

**ATCP 50.70** **Diversions.**

[ATCP 50.70(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.70%281%29) **(1)**  Definition. In this section, “diversion" means a structure installed to divert excess surface runoff water to an area where it can be used, transported, or discharged without causing excessive soil erosion. “Diversion" includes a channel with a supporting earthen ridge on the lower side, installed across the slope with a self-discharging and non-erosive gradient.

**ATCP 50.705** **Feed storage runoff control systems.**

[ATCP 50.705(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.705%281%29)**(1)**  Definitions. In this section:

[ATCP 50.705(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.705%281%29%28a%29) **(a)** “Feed storage area" means an area used to store livestock feed including corn silage, haylage, and industrial by-products including distillers grain, brewers grain, candy, pizza crust, bakery waste, cotton seed, soybean meal, animal fats, blood meal, fish meal, cannery waste, beet pulp, citrus pulp, soy hulls, corn middlings, whey, potatoes, and grocery store vegetables. The feed storage area includes the area up to the outside edge of the surface on which the feed is stored and any apron area.

[ATCP 50.705(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.705%281%29%28b%29) **(b)** “Feed storage runoff control system" means a system of facilities or practices to contain, divert, retard, treat, or otherwise control the discharge of leachate and contaminated runoff from livestock feed storage areas.

**ATCP 50.71** **Field windbreaks.**

[ATCP 50.71(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.71%281%29) **(1)**  Definition. In this section, “field windbreak" means a strip or belt of trees, shrubs, or grasses established or renovated within or adjacent to a field, so as to control soil erosion by reducing wind velocities at the land surface.

**ATCP 50.72** **Filter strips.**

[ATCP 50.72(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.72%281%29) **(1)**  Definition. In this section:

[ATCP 50.72(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.72%281%29%28a%29) **(a)** “Filter strip" means an area of herbaceous vegetation that separates an environmentally sensitive area from cropland, grazing land, or disturbed land. “Filter strip" does not include a wastewater treatment strip.

[ATCP 50.72(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.72%281%29%28b%29) **(b)** “Wastewater treatment strip" has the meaning given in s. [ATCP 50.94 (1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.94%281%29).

**ATCP 50.73** **Grade stabilization structures.**Down

[ATCP 50.73(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.73%281%29) **(1)**  Definition. In this section, “grade stabilization structure" means a structure which stabilizes the grade in a channel in order to protect the channel from erosion, or to prevent gullies from forming or advancing. A “grade stabilization structure" may include any of the following:

[ATCP 50.73(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.73%281%29%28a%29) **(a)** Detention or retention structures such as dams, desilting reservoirs, sediment basins, and debris basins.

[ATCP 50.73(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.73%281%29%28b%29) **(b)** Related structures such as channel linings, chutes, drop spillways, or pipe drops.

**ATCP 50.75** **Livestock fencing.**

[ATCP 50.75(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.75%281%29) **(1)**  Definition. In this section, “livestock fencing" means either of the following:

[Down](https://docs.legis.wisconsin.gov/scroll/down/1472/code/admin_code/atcp/020/50)

[Up](https://docs.legis.wisconsin.gov/scroll/up/1473/code/admin_code/atcp/020/50)

[ATCP 50.75(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.75%281%29%28a%29) **(a)** Excluding livestock, by fencing or other means, in order to protect an erodible area or a practice under this subchapter.

[ATCP 50.75(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.75%281%29%28b%29) **(b)** Restricting, by fencing or other means, human access to manure storage structures or other practices under this subchapter which may pose a hazard to humans.

**ATCP 50.76** **Livestock watering facilities.**

[ATCP 50.76(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.76%281%29) **(1)**  Definition. In this section, “livestock watering facility" means a trough, tank, pipe, conduit, spring development, pump, well, or other device or combination of devices installed to deliver drinking water to livestock.

**ATCP 50.77** **Milking center waste control systems.**

[ATCP 50.77(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.77%281%29)**(1)**  Definitions. In this section:

[ATCP 50.77(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.77%281%29%28a%29) **(a)** “Milking center waste" means waste water, cleaning ingredients, waste milk, or other discharge from a milking parlor or milkhouse.

[ATCP 50.77(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.77%281%29%28b%29) **(b)** “Milking center waste control system" means a system of facilities or equipment designed to contain or control the discharge of milking center waste.

**ATCP 50.78** **Nutrient management.**

[ATCP 50.78(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.78%281%29) **(1)**  Definitions. In this section, “nutrient management" means controlling the amount, source, form, location, and timing of plant nutrient applications, including application of organic wastes, commercial fertilizers, soil reserves, and legumes, in order to provide plant nutrients while minimizing the movement of nutrients to surface water and groundwater.

**ATCP 50.79** **Pesticide management.**

[ATCP 50.79(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.79%281%29) **(1)**  Definition. In this section, “pesticide management" means controlling the storage, handling, use, and disposal of pesticides used in crop production in order to minimize contamination of water, air, and nontarget organisms.

**ATCP 50.80** **Prescribed grazing.**

[ATCP 50.80(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.80%281%29) **(1)**  Definition. In this section, “prescribed grazing" or “rotational grazing" means a grazing system which divides pastures into multiple cells, each of which is grazed intensively for a short period and then protected from grazing until its vegetative cover is restored.

ATCP 50.80 Note **Note:** Prescribed grazing systems can prevent degradation resulting from other pasturing practices. Prescribed grazing systems should replace summer dirt lots when they result in water quality degradation.

**ATCP 50.81** **Relocating or abandoning animal feeding operations.**

[ATCP 50.81(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29)**(1)**  Definitions. In this section:

[ATCP 50.81(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29%28a%29) **(a)** “Abandonment" means discontinuing an animal feeding operation in order to prevent surface water or groundwater pollution from that animal feeding operation.

[ATCP 50.81(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29%28b%29) **(b)** “Animal feeding operation" means a feedlot or facility, other than a pasture, where animals are fed, confined, maintained, or stabled for 45 days or more in any 12-month period. Two or more animal feeding operations under common ownership or common management constitute a single animal feeding operation if any of the following apply:

[ATCP 50.81(1)(b)1.](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29%28b%291.) **1.** The operations are adjacent.

[ATCP 50.81(1)(b)2.](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29%28b%292.) **2.** The operations use common plans, acreage, or systems to landspread manure or other wastes.

[ATCP 50.81(1)(b)3.](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29%28b%293.) **3.** Manure, barnyard runoff, or other wastes are commingled in a common storage facility prior to landspreading.

[ATCP 50.81(1)(c)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.81%281%29%28c%29) **(c)** “Relocation" means discontinuing an animal feeding operation at one site and commencing that operation at a suitable alternate site in order to minimize the amount of surface water or groundwater pollution from that animal feeding operation.

**ATCP 50.82** **Residue management.**

[ATCP 50.82(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.82%281%29) **(1)**  Definition. In this section, “residue management" means any of the following:

[ATCP 50.82(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.82%281%29%28a%29) **(a)** Preparing land surfaces for the planting and growing of crop plants using methods that result in a rough land surface which is covered in varying degrees by vegetative residues of a previous crop, and which provides a significant degree of resistance to soil erosion by raindrop impact, surface water runoff, or wind.

[ATCP 50.82(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.82%281%29%28b%29) **(b)** Planting crop seeds in a narrow slot or a narrow strip of tilled soil, in order to maintain residue cover and avoid disturbing the entire soil surface.

**ATCP 50.83** **Riparian buffers.**

[Down](https://docs.legis.wisconsin.gov/scroll/down/1646/code/admin_code/atcp/020/50)

[Up](https://docs.legis.wisconsin.gov/scroll/up/1647/code/admin_code/atcp/020/50)

[ATCP 50.83(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.83%281%29) **(1)**  Definition. In this section, “riparian buffer" means an area in which vegetation is enhanced or established to reduce or eliminate the movement of sediment, nutrients, and other nonpoint source pollutants to an adjacent surface water resource or groundwater recharge area, to protect the banks of streams and lakes from erosion, and to protect fish habitat.

**ATCP 50.84** **Roofs.**

[ATCP 50.84(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.84%281%29) **(1)**  Definitions. In this section:

[ATCP 50.84(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.84%281%29%28a%29) **(a)** “Roof" means a weather-proof covering that shields an animal lot or manure storage structure from precipitation, and includes the structure supporting that weather-proof covering. “Roof" does not include, except in the case of a manure storage structure, a covering over an enclosed structure if the sum of the length of the walls of the structure exceeds 50% of the perimeter of the covering. If a structure includes 2 or more square or rectangular areas, the ratio of wall length to covering perimeter shall be separately calculated for each square or rectangular area, excluding common sides.

[ATCP 50.84(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.84%281%29%28b%29) **(b)** “Wall" means a vertical expanse in which more than 50% of the opening from eave to floor or ground is composed of a solid building material. The building material need not be rigid.

**ATCP 50.85** **Roof runoff systems.**

[ATCP 50.85(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.85%281%29) **(1)**  Definition. In this section, “roof runoff system" means facilities for collecting, controlling, diverting, and disposing of precipitation from roofs. A “roof runoff system" may include gutters, downspouts, erosion-resistant channels, subsurface drains, and trenches.

**ATCP 50.86** **Sediment basins.**

[ATCP 50.86(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.86%281%29) **(1)**  Definition. In this section:

[ATCP 50.86(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.86%281%29%28a%29) **(a)** “Sediment basins" means permanent basins that reduce the transport of waterborne pollutants such as eroded soil sediment, debris, and manure sediment. Sediment basins may include containment walls or berms, pickets or screens to filter debris, orifices or weirs to control discharge, and conduits to direct runoff to treatment or discharge areas.

[ATCP 50.86(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.86%281%29%28b%29) **(b)** “Maximum storage capacity" means the volume of water, in acre-feet, capable of being stored behind a dam at maximum water elevation without overtopping any part that is not part of the spillway system.

**ATCP 50.87** **Sinkhole treatment.**

[ATCP 50.87(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.87%281%29) **(1)**  Definition. In this section, “sinkhole treatment" means modifying a sinkhole, or the area around a sinkhole, to reduce erosion, prevent expansion of the hole, and reduce pollution of water resources. Modifications may include the diversion of runoff around a sinkhole, or the alteration of a sinkhole by excavation, cleanout, filter treatment, sealing, or refilling.

[ATCP 50.87(2)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.87%282%29) **(2)** Eligible costs. A cost-share grant under s. [ATCP 50.40](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.40) may reimburse any of the following costs related to sinkhole treatment:

[ATCP 50.87(2)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.87%282%29%28a%29) **(a)** Costs for the design and construction of a grassed waterway or diversion to direct surface runoff around a sinkhole.

[ATCP 50.87(2)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.87%282%29%28b%29) **(b)** Costs for the design and construction of a grassed waterway or diversion to direct surface runoff around a geologic depression to prevent the formation of a sinkhole.

[ATCP 50.87(2)(c)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.87%282%29%28c%29) **(c)** Costs for the design and construction of a modification to a sinkhole for the purpose of protecting groundwater resources from contamination.

**ATCP 50.88** **Streambank or shoreline protection.**

[ATCP 50.88(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29)**(1)**  Definition. In this section, “streambank or shoreline protection" means waterbody-specific treatments used to stabilize and protect the eroding banks of streams or constructed channels, and shorelines of lakes, reservoirs, or estuaries. The practice is designed and installed to provide water quality benefits or control soil erosion including degradation from livestock and may protect fish habitat as an incidental benefit. Streambank or shoreline protection may include any of the following components:

[ATCP 50.88(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28a%29) **(a)** Critical area stabilization under s. [ATCP 50.69](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.69).

[ATCP 50.88(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28b%29) **(b)** Diversions under s. [ATCP 50.70](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.70).

[Down](https://docs.legis.wisconsin.gov/scroll/down/1733/code/admin_code/atcp/020/50)

[Up](https://docs.legis.wisconsin.gov/scroll/up/1734/code/admin_code/atcp/020/50)

[ATCP 50.88(1)(c)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28c%29) **(c)** Grade stabilization under s. [ATCP 50.73](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.73).

[ATCP 50.88(1)(d)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28d%29) **(d)** Riparian buffers under s. [ATCP 50.83](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.83).

[ATCP 50.88(1)(e)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28e%29) **(e)** Roof runoff systems under s. [ATCP 50.85](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.85).

[ATCP 50.88(1)(f)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28f%29) **(f)** Subsurface drain under s. [ATCP 50.90](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.90).

[ATCP 50.88(1)(g)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28g%29) **(g)** Underground outlet under s. [ATCP 50.92](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.92).

[ATCP 50.88(1)(h)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.88%281%29%28h%29) **(h)** Wetland development or restoration under s. [ATCP 50.98](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.98).

**ATCP 50.885** **Stream Crossing.**

[ATCP 50.885(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.885%281%29) **(1)**  Definition. In this section, “stream crossing" means a road or pathway which confines or directs the movement of livestock, farm equipment, or vehicular traffic over a stream, and which is designed and installed to improve water quality, reduce erosion, protect an installed practice, or control livestock access to a stream.

[ATCP 50.885(2)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.885%282%29) **(2)** Eligible costs. A cost-share grant under s. [ATCP 50.40](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.40) may reimburse any of the following costs related to a stream crossing:

[ATCP 50.885(2)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.885%282%29%28a%29) **(a)** The costs of constructing a culvert, ford, or other allowed stream crossing structure other than a bridge.

[ATCP 50.885(2)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.885%282%29%28b%29) **(b)** The costs of installing conservation practices necessary to limit water quality impairment from a stream crossing.

**ATCP 50.89** **Stripcropping.**

[ATCP 50.89(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.89%281%29) **(1)**  Definition. In this section, “stripcropping" means growing crops in a systematic strip arrangement in which strips of grass, legumes, or other close growing crops are alternated with strips of clean tilled crops or fallow, and in which all of the strips are established on the contour or across a slope to reduce water or wind erosion.

**ATCP 50.90** **Subsurface drains.**

[ATCP 50.90(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.90%281%29) **(1)**  Definition. In this section, “subsurface drain" means a conduit installed below the surface of the ground to collect drainage water and convey it to a suitable outlet.

**ATCP 50.91** **Terrace systems.**

[Down](https://docs.legis.wisconsin.gov/scroll/down/1791/code/admin_code/atcp/020/50)

[Up](https://docs.legis.wisconsin.gov/scroll/up/1792/code/admin_code/atcp/020/50)

[ATCP 50.91(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.91%281%29) **(1)**  Definition. In this section, “terrace system" means a system of ridges and channels installed on the contour with a non-erosive grade and suitable spacing.

**ATCP 50.92** **Underground outlets.**

[ATCP 50.92(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.92%281%29) **(1)**  Definition. In this section, “underground outlet" means a conduit installed below the surface of the ground to collect surface water and convey it to a suitable outlet.

**ATCP 50.93** **Waste transfer systems.**

[ATCP 50.93(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.93%281%29) **(1)**  Definition. In this section, “waste transfer system" means components such as pumps, pipes, conduits, valves, and other structures installed to convey manure and milking center wastes from buildings and animal feeding operations to a storage structure, loading area, or treatment area.

**ATCP 50.94** **Wastewater treatment strips.**

[ATCP 50.94(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.94%281%29) **(1)**  Definition. In this section, “wastewater treatment strip" means an area of herbaceous vegetation that is used as part of an agricultural waste management system to remove pollutants from animal lot runoff or wastewater, such as runoff or wastewater from a milking center.

**ATCP 50.95** **Water and sediment control basins.**

[ATCP 50.95(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.95%281%29)**(1)**  Definitions. In this section:

[Down](https://docs.legis.wisconsin.gov/scroll/down/1849/code/admin_code/atcp/020/50)

[Up](https://docs.legis.wisconsin.gov/scroll/up/1850/code/admin_code/atcp/020/50)

[ATCP 50.95(1)(a)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.95%281%29%28a%29) **(a)** “Manure storage facility" has the meaning given in s. [ATCP 50.62 (1) (c)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.62%281%29%28c%29).

[ATCP 50.95(1)(b)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.95%281%29%28b%29) **(b)** “Water and sediment control basin" means an earthen embankment or a ridge and channel combination which is installed across a slope or minor watercourse to trap or detain runoff and sediment. “Water and sediment control basin" does not include a manure storage facility or a structure designed to collect runoff and sediment from concentrated animal feedlots.

**ATCP 50.96** **Waterway systems.**

[ATCP 50.96(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.96%281%29) **(1)**  Definition. In this section, “waterway system" means a natural or constructed waterway or outlet that is shaped, graded, and covered with a vegetation or another suitable surface material to prevent erosion by runoff waters.

**ATCP 50.97** **Well decommissioning.**

[ATCP 50.97(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.97%281%29) **(1)**  Definition. In this section, “well decommissioning" means permanently disabling and sealing a well to prevent contaminants from reaching groundwater.

**ATCP 50.98** **Wetland development or restoration.**

[ATCP 50.98(1)](https://docs.legis.wisconsin.gov/document/administrativecode/ATCP%2050.98%281%29)**(1)**  Definition. In this section, “wetland development or restoration" means the construction of berms, or the destruction of tile line or drainage ditch functions, to create or restore conditions suitable for wetland vegetation.